[42] BODY - - KEYLESS ENTRY SYSTEM - ON-VEHICLE SERVICE - ENABLING/DISABLING THE ANSWERBACK FUNCTION <EXCEPT VEHICLES FOR HONG KONG SPEC> | PRINT PAGE / INDEX / PRIOR / NEXT

| ENABLING/DISABLING THE ANSWERBACK FUNCTION <EXCEPT VEHICLES FOR HONG KONG SPEC>
| If the keyless entry system locks or unlocks the doors, the room lamp flashes or illuminates, the hazard warning lamp flashes (hazard answerback function). The hazard answerback function can be enabled or disabled according to the following procedure:
| ENABLING/DISABLING THE HAZARD ANSWERBACK FUNCTION The hazard answerback function can be enabled or disabled by one of the two following procedures.
| <WHEN USING THE TRANSMITTER AFTER DIAGNOSIS CONNECTOR (1) IS EARTHED> Enter the hazard answerback customize mode by performing one of the following steps. If the ETACS-ECU enters the customize mode, its buzzer will sound once. Turn the ignition switch to “LOCK”(OFF) position. Turn off the hazard warning lamp switch. CAUTION Before connecting or disconnecting the earth, turn the ignition switch to the "LOCK" (OFF) position.
| Connect the diagnosis connector to the special tool diagnosis code check harness (MB991529). Close the driver's side door. Keep the windshield washer switch on for at least ten seconds. Then the ETACS-ECU buzzer will sound once. If the transmitter “LOCK” button is pushed consecutively twice (within two seconds), the ETACS-ECU buzzer will sound, indicating that the hazard answerback function can be enabled or disabled when the doors are locked. Enable the hazard answerback function when the doors are locked: The ETACS-ECU buzzer will sound once. Disable the hazard answerback function when the doors are locked: The ETACS-ECU buzzer will sound twice. If the transmitter “UNLOCK” button is pushed consecutively twice (within two seconds), the ETACS-ECU buzzer will sound, indicating that the hazard answerback function can be enabled or disabled when the doors are unlocked. Enable the hazard answerback function when the doors are unlocked: The ETACS-ECU buzzer will sound once. Disable the hazard answerback function when the doors are unlocked: The ETACS-ECU buzzer will sound twice. Exit the hazard answerback customize mode by observing one of the following steps. Disconnect diagnosis connector terminal (1) form the earth. Turn the ignition switch to position other then “LOCK”(OFF), or remove the ignition key. Open the driver's side door, Any other warning buzzer output occurs. NOTE: If any operation is not done for at least three minutes after the ETACS-ECU has entered the customize mode, the hazard answerback customize mode will be cancelled automatically.
| <WHEN THE TRANSMITTER IS USED AFTER CONNECTING MUT-II TO THE DIAGNOSIS CONNECTOR> Enter the hazard answerback customize mode by performing one of the following steps. If the ETACS-ECU enters the customize mode, its buzzer will sound once. Turn the ignition switch to “LOCK”(OFF) position. Turn off the hazard warning lamp switch. CAUTION Before connecting or disconnecting the MUT-II, turn the ignition switch to the "LOCK" (OFF) position.
| Connect the MUT-II to the diagnosis connector. Close the driver's side door. Keep the windshield washer switch on for at least ten seconds. Then the ETACS-ECU buzzer will sound once. If the transmitter “LOCK” button is pushed consecutively twice (within two seconds), the ETACS-ECU buzzer will sound, indicating that the hazard answerback function can be enabled or disabled when the doors are locked. Enable the hazard answerback function when the doors are locked: The ETACS-ECU buzzer will sound once. Disable the hazard answerback function when the doors are locked: The ETACS-ECU buzzer will sound twice. If the transmitter “UNLOCK” button is pushed consecutively twice (within two seconds), the ETACS-ECU buzzer will sound, indicating that the hazard answerback function can be enabled or disabled when the doors are unlocked. Enable the hazard answerback function when the doors are unlocked: The ETACS-ECU buzzer will sound once. Disable the hazard answerback function when the doors are unlocked: The ETACS-ECU buzzer will sound twice. Exit the hazard answerback customize mode by observing one of the following steps. Disconnect MUT-II from the diagnosis connector. Turn the ignition switch to position other then “LOCK”(OFF), or remove the ignition key. Open the driver's side door, Any other warning buzzer output occurs. NOTE: If any operation is not done for at least three minutes after the ETACS-ECU has entered the customize mode, the hazard answerback customize mode will be cancelled automatically.
| <WHEN THE TRANSMITTER IS USED AFTER CONNECTING SPECIAL TOOL V. C. I. (MB991824) TO THE DIAGNOSIS CONNECTOR> Enter the hazard answerback customize mode by performing one of the following steps. If the ETACS-ECU enters the customize mode, its buzzer will sound once. Turn the ignition switch to “LOCK”(OFF) position. Turn off the hazard warning lamp switch. CAUTION Before connecting or disconnecting the V. C. I., turn the ignition switch to the "LOCK" (OFF) position.
| Connect the V. C. I. to the diagnosis connector. Turn the V.C.I. power switch to the "ON" position. Close the driver's side door. Keep the windshield washer switch on for at least ten seconds. Then the ETACS-ECU buzzer will sound once. If the transmitter “LOCK” button is pushed consecutively twice (within two seconds), the ETACS-ECU buzzer will sound, indicating that the hazard answerback function can be enabled or disabled when the doors are locked. Enable the hazard answerback function when the doors are locked: The ETACS-ECU buzzer will sound once. Disable the hazard answerback function when the doors are locked: The ETACS-ECU buzzer will sound twice. If the transmitter “UNLOCK” button is pushed consecutively twice (within two seconds), the ETACS-ECU buzzer will sound, indicating that the hazard answerback function can be enabled or disabled when the doors are unlocked. Enable the hazard answerback function when the doors are unlocked: The ETACS-ECU buzzer will sound once. Disable the hazard answerback function when the doors are unlocked: The ETACS-ECU buzzer will sound twice. Exit the hazard answerback customize mode by observing one of the following steps. Disconnect V. C. I. from the diagnosis connector. Turn the ignition switch to position other then “LOCK”(OFF), or remove the ignition key. Open the driver's side door. Any other warning buzzer output occurs. NOTE: If any operation is not done for at least three minutes after the ETACS-ECU has entered the customize mode, the hazard answerback customize mode will be cancelled automatically.

[42] BODY - - KEYLESS ENTRY SYSTEM - ON-VEHICLE SERVICE - ENABLING/DISABLING THE ANSWERBACK FUNCTION <EXCEPT VEHICLES FOR HONG KONG SPEC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation