[2] BODY DIMENSIONS - - TYPE B (ACTUAL-MEASUREMENT DIMENSIONS) - FRONT BODY <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

FRONT BODY <2400>
No. | Standard measurement point | Hole shape | Size mm
--- | --- | --- | ---
23 | Centre of front end crossmember upper water draining hole (Body centre point) | Round | 9
24 | Centre of harness mounting hole | Oblong | 7 × 12
25 | Centre of intercooler pipe mounting hole | Round | 9
26 | Centre of front fender mounting hole | Round | 6.6
27 | Centre of front strut mounting hole | Round | 11.5
28 | Centre of cowl top panel positioning hole (Body centre point) | Oblong | 7 × 5
29 | Centre of front fender mounting hole | Round | 6.6
30 | Centre of hood hinge mounting hole | Round | 9
31 | Corner of roof panel | - | -
32 | Centre of front end crossmember outer positioning hole | Round | 20
33 | Centre of front bumper mounting hole | Round | 9
34 | Centre of headlamp mounting hole | Round | 6.6
35 | Centre of hood latch mounting hole (Body centre point) | Round | 6.6

[2] BODY DIMENSIONS - - TYPE B (ACTUAL-MEASUREMENT DIMENSIONS) - FRONT BODY <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation