[37] POWER STEERING - - POWER STEERING HOSES - REMOVAL AND INSTALLATION <L.H. DRIVE VEHICLES> | PRINT PAGE / INDEX / PRIOR / NEXT

POWER STEERING HOSES

REMOVAL AND INSTALLATION <L.H. DRIVE VEHICLES>
Pre-removal and Post-installation Operation Power Steering Fluid Draining and Refilling (Refer to ). and Bleeding (Refer to ).
<2400 (Except MIVEC)>
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Oil reservoir
| >>F<< | 2. | Return hose
| >>E<< | 3. | Suction hose
| >>D<< | 4. | Return hose
| >>C<< | 5. | Return hose
| >>B<< | 6. | Return hose
|  | 7. | Return tube assembly
|  | • | Front bumper assembly (Refer to GROUP 51, Front Bumper Assembly <2400>).
|  | 8. | Cooler tube assembly
|  | • | Tie rod end and knuckle connection (Refer to ).
|  | • | Stabilizer link (Refer to GROUP 33, Stabilizer Bar <2000-DOHC and 2400 >).
| >>A<< | 9. | Return hose
|  | 10. | Return tube
|  | 11. | O-ring
|  | 12. | Eye bolt
|  | 13. | Gasket
|  | 14. | Pressure hose assembly
|  | 15. | Return tube
<2400 (MIVEC)>
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Oil reservoir
| >>F<< | 2. | Return hose
| >>E<< | 3. | Suction hose
| >>D<< | 4. | Return hose
| >>C<< | 5. | Return hose
| >>B<< | 6. | Return hose
|  | 7. | Return tube assembly
|  | • | Front bumper assembly (Refer to GROUP 51, Front Bumper Assembly <2400>).
|  | 8. | Cooler tube assembly
|  | • | Tie rod end and knuckle connection (Refer to ).
|  | • | Stabilizer link (Refer to GROUP 33, Stabilizer Bar <2000-DOHC and 2400 >).
| >>A<< | 9. | Return hose
|  | 10. | Return tube
|  | 11. | O-ring
|  | 12. | Eye bolt
|  | 13. | Gasket
|  | 14. | Pressure hose assembly
|  | 15. | Return tube
| INSTALLATION SERVICE POINTS
| >>A<< RETURN HOSE INSTALLATION
| Install the return hose so that the marking is positioned as shown in the illustration.
| >>B<< RETURN HOSE INSTALLATION
| Install the return hose so that the marking is positioned as shown in the illustration.
| >>C<< RETURN HOSE INSTALLATION
| Install the return hose so that the marking is positioned as shown in the illustration.
| >>D<< RETURN HOSE INSTALLATION
| Install the return hose so that the markings are positioned as shown in the illustration.
| >>E<< SUCTION HOSE INSTALLATION
| Install the suction hose so that the marking is positioned as shown in the illustration.
| >>F<< RETURN HOSE INSTALLATION
| Install the return hose so that the markings are positioned as shown in the illustration.

[37] POWER STEERING - - POWER STEERING HOSES - REMOVAL AND INSTALLATION <L.H. DRIVE VEHICLES> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation