[42] BODY - - DOOR - DOOR GLASS AND REGULATOR - INSPECTION <VEHICLES FOR HONG KONG SPEC AND ARGENTINA> | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION <VEHICLES FOR HONG KONG SPEC AND ARGENTINA>
| HOW TO MAKE THE POWER WINDOW SWITCH LEARN THE FULLY CLOSED POSITION OF THE POWER WINDOW
| HOW TO MAKE THE POWER WINDOW SWITCH LEARN THE FULLY CLOSED POSITION WHEN THE POWER WINDOW SWITCH IS REMOVED, OR THE POWER WINDOW REGULATOR ASSEMBLY IS REMOVED OR REPLACED If the anti-trap function (safety mechanism) is activated consecutively three times or more, the fully closed position that the power window switch has learned will be erased (initialised). Operate the power window switch and fully open the door window glass. CAUTION The anti-trap function does not work until the power window switch completes learning the fully closed position. (It is because the anti-trap function is reset.) Operate the power window switch and fully close the door window glass. The power window activates for 0.7 seconds and stops automatically when the power window switch is pressed once. Repeat this operation until the door window glass fully closes and release the switch once. Then, hold the power window switch to the fully closed side again for one second so that the power window switch completes learning the fully closed position. NOTE: If the power window switch is operated to open the door window glass while the switch is learning, learning will be cancelled. If this happens, return to step 2.
| HOW TO MAKE THE POWER WINDOW SWITCH LEARN THE FULLY CLOSED POSITION WHEN THE POWER WINDOW SWITCH IS REPLACED WITH A NEW ONE CAUTION The anti-trap function does not work until the power window switch completes learning the fully closed position. (It is because the anti-trap function is reset.) Operate the power window main switch to fully close the door window glass by one-shot up action so that the power window switch will complete learning. (Initialisation is not needed.) NOTE: When the power window sub switch of each seat is replaced, operate the power window main switch to fully close the applicable power window by one-shot up action. (It is because the power window sub switch does not have one-shot up/down function.)

[42] BODY - - DOOR - DOOR GLASS AND REGULATOR - INSPECTION <VEHICLES FOR HONG KONG SPEC AND ARGENTINA> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation