[0] GENERAL - - MAJOR SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

MAJOR SPECIFICATIONS
VEHICLES FOR GENERAL EXPORT
(Except for Hong Kong spec., Brazil, South Africa and Argentina)
Items | CU4W | CU5W
--- | --- | ---
XRHEZL/R | XRMYZL | XRHYZL | XRHJZL
Vehicle dimension mm | Overall length | 4,545
Overall width | 1,750/1,780*1
Overall height (unladen) | 1,630/1,680*2
Wheelbase | 2,625
Track | Front | 1,495
Rear | 1,505
Front overhang | 945
Rear overhang | 975
Ground clearance (unladen) | 205
Vehicle wheel alignment | Front | Toe-in (at the centre of tyre tread) mm | 1 ± 2
Toe angle (per wheel) | 0°00' ± 05'
Toe-out angle on turns (inner wheel when outer wheel at 20°) | 22°00' ± 1°30'
Camber*3 | 0°00' ± 30'
Caster*3 | 3°10' ± 30'
Kingpin inclination angle | 12°05' ± 1°30'
Side slip (per 1m) mm | 0 ± 3
Steering angle | Inner wheels | 34°50' ± 1°30'
Outer wheels (reference) | 29°20'
Rear | Toe-in (at the centre of tyre tread) mm | 3 ± 2
Toe angle (per wheel) | 0°08' ± 05'
Camber | -0°40' ± 30'
Wheels and tyres | Tyre size | 215/60 R16 95H
Wheel size | 16 × 6JJ
Offset mm | 46
NOTE: *1 : Vehicles with over fender. *2 : Vehicles with roof rails. *3 : Difference between right and left wheels must be less than 30'.
(For Hong Kong, Brunei, Singapore, Maiaysia)
Items | CU2W | CU5W
--- | --- | ---
LRMER1D | LYXFZR1D | XRHYZR1D
Vehicle dimension mm | Overall length | 4,465 | 4,550
Overall width | 1,750 | 1,780
Overall height (unladen) | 1,550/1,585*1 | 1,540/1,575*1 | 1,685
Wheelbase | 2,625
Track | Front | 1,495
Rear | 1,495 | 1,505
Front overhang | 900 | 950
Rear overhang | 940 | 975
Ground clearance (unladen) | 195 | 160 | 205
Vehicle wheel alignment | Front | Toe-in (at the centre of tyre tread) mm | 1 ± 2
Toe angle (per wheel) | 0°00' ± 05'
Toe-out angle on turns (inner wheel when outer wheel at 20°) | 22°00' ± 1°30'
Camber*2 | -0°05' ± 30' | -0°15' ± 30' | 0°00' ± 30'
Caster*2 | 3°30' ± 30' | 3°35' ± 30' | 3°10' ± 30'
Kingpin inclination angle | 12°55' ± 1°30' | 13°10' ± 1°30' | 12°05' ± 1°30'
Side slip (per 1m) mm | 0 ± 3
Steering angle | Inner wheels | 34°20' ± 1°30' | 34°50' ± 1°30'
Outer wheels (reference) | 29°10' | 29°20'
Rear | Toe-in (at the centre of tyre tread) mm | 3 ± 2
Toe angle (per wheel) | 0°08' ± 05'
Camber | -0°40' ± 30'
Wheels and tyres | Tyre size | 215/60 R16 95H
Wheel size | 16 × 6JJ
Offset mm | 46
NOTE: *1 : Vehicles with roof rails. *2 : Difference between right and left wheels must be less than 30'.
(For Brazil)
Items | CU5W
--- | ---
XRMYZL1F | XRHYZL1F
Vehicle dimension mm | Overall length | 4,545
Overall width | 1,750/1,780*1
Overall height (unladen) | 1,630/1,680*2
Wheelbase | 2,625
Track | Front | 1,495
Rear | 1,505
Front overhang | 945
Rear overhang | 975
Ground clearance (unladen) | 205
Vehicle wheel alignment | Front | Toe-in (at the centre of tyre tread) mm | 1 ± 2
Toe angle (per wheel) | 0°00' ± 05'
Toe-out angle on turns (inner wheel when outer wheel at 20°) | 22°00' ± 1°30'
Camber*3 | 0°00' ± 30'
Caster*3 | 3°10' ± 30'
Kingpin inclination angle | 12°05' ± 1°30'
Side slip (per 1m) mm | 0 ± 3
Steering angle | Inner wheels | 34°50' ± 1°30'
Outer wheels (reference) | 29°20'
Rear | Toe-in (at the centre of tyre tread) mm | 3 ± 2
Toe angle (per wheel) | 0°08' ± 05'
Camber | -0°40' ± 30'
Wheels and tyres | Tyre size | 215/60 R16 95H
Wheel size | 16 × 6JJ
Offset mm | 46
NOTE: *1 : Vehicles with over fender. *2 : Vehicles with roof rails. *3 : Difference between right and left wheels must be less than 30'.
(For South Africa and Argentina)
Items | CU5W
--- | ---
XRMYZR6S | XRHYZR6S | XRHYZL6A
Vehicle dimension mm | Overall length | 4,545
Overall width | 1,750/1,780*1 | 1,780
Overall height (unladen) | 1,620/1,670*2 | 1,670
Wheelbase | 2,625
Track | Front | 1,495
Rear | 1,505
Front overhang | 945
Rear overhang | 975
Ground clearance (unladen) | 195
Vehicle wheel alignment | Front | Toe-in (at the centre of tyre tread) mm | 1 ± 2
Toe angle (per wheel) | 0°00' ± 05'
Toe-out angle on turns (inner wheel when outer wheel at 20°) | 22°00' ± 1°30'
Camber*3 | 0°00' ± 30'
Caster*3 | 3°10' ± 30'
Kingpin inclination angle | 12°05' ± 1°30'
Side slip (per 1m) mm | 0 ± 3
Steering angle | Inner wheels | 34°50' ± 1°30'
Outer wheels (reference) | 29°20'
Rear | Toe-in (at the centre of tyre tread) mm | 3 ± 2
Toe angle (per wheel) | 0°08' ± 05'
Camber | -0°40' ± 30'
Wheels and tyres | Tyre size | 215/60 R16 95H
Wheel size | 16 × 6JJ
Offset mm | 46
NOTE: *1 : Vehicles with over fender. *2 : Vehicles with roof rails. *3 : Difference between right and left wheels must be less than 30'.
VEHICLES FOR GCC
Items | CU5W
--- | ---
XRMYZLW | XRHYZLW
Vehicle dimension mm | Overall length | 4,545
Overall width | 1,750/1,780*1
Overall height (unladen) | 1,630/1,680*2
Wheelbase | 2,625
Track | Front | 1,495
Rear | 1,505
Front overhang | 945
Rear overhang | 975
Ground clearance (unladen) | 205
Vehicle wheel alignment | Front | Toe-in (at the centre of tyre tread) mm | 1 ± 2
Toe angle (per wheel) | 0°00' ± 05'
Toe-out angle on turns (inner wheel when outer wheel at 20°) | 22°00' ± 1°30'
Camber*3 | 0°00' ± 30'
Caster*3 | 3°10' ± 30'
Kingpin inclination angle | 12°05' ± 1°30'
Side slip (per 1m) mm | 0 ± 3
Steering angle | Inner wheels | 34°50' ± 1°30'
Outer wheels (reference) | 29°20'
Rear | Toe-in (at the centre of tyre tread) mm | 3 ± 2
Toe angle (per wheel) | 0°08' ± 05'
Camber | -0°40' ± 30'
Wheels and tyres | Tyre size | 215/60 R16 95H
Wheel size | 16 × 6JJ
Offset mm | 46
NOTE: *1 : Vehicles with over fender. *2 : Vehicles with roof rails. *3 : Difference between right and left wheels must be less than 30'.
VEHICLES FOR NEW ZEALAND
Items | CU2W | CU5W
--- | --- | ---
LRMER1D | LYXFZR1D | XRMYZR8, XRHYZR8 | XRXYZR8
Vehicle dimension mm | Overall length | 4,465 | 4,550
Overall width | 1,750 | 1,750/1,780*1
Overall height | 1,550/1,585*2 | 1,540/1,575*2 | 1,630/1,680*2
Wheelbase | 2,625
Track | Front | 1,495
Rear | 1,495 | 1,505
Front overhang | 900 | 945
Rear overhang | 940 | 975
Ground clearance | 195 | 160 | 205
Vehicle wheel alignment | Front | Toe-in (at the centre of tyre tread) mm | 1 ± 2
Toe angle (per wheel) | 0°00' ± 05'
Toe-out angle on turns (inner wheel when outer wheel at 20°) | 22°00' ± 1°30'
Camber*3 | -0°05' ± 30' | -0°15' ± 30' | 0°00' ± 30'
Caster*3 | 3°30' ± 30' | 3°35' ± 30' | 3°10' ± 30'
Kingpin inclination angle | 12°55' ± 1°30' | 13°10' ± 1°30' | 12°05' ± 1°30'
Side slip (per 1m) mm | 0 ± 3
Steering angle | Inner wheels | 34°20' ± 1°30' | 34°50' ± 1°30'
Outer wheels (reference) | 29°10' | 29°20'
Rear | Toe-in (at the centre of tyre tread) mm | 3 ± 2
Toe angle (per wheel) | 0°08' ± 05'
Camber | -0°40' ± 30'
Wheels and tyres | Tyre size | 215/60 R16 95H | 215/55 R17 94V
Wheel size | 16 × 6JJ | 17 × 6.5JJ
Offset mm | 46 | 38
NOTE: *1 : Vehicles with over fender. *2 : Vehicles with roof rails. *3 : Difference between right and left wheels must be less than 30'.
VEHICLES FOR AUSTRALIA
Items | CU5W
--- | ---
XRMYZR8 | XRHYZR8 | XRXYZR8
Vehicle dimension mm | Overall length | 4,550
Overall width | 1,750/1,780*1
Overall height | 1,635/1,685*2
Wheelbase | 2,625
Track | Front | 1,495
Rear | 1,505
Front overhang | 945
Rear overhang | 975
Ground clearance | 210
Vehicle wheel alignment | Front | Toe-in (at the centre of tyre tread) mm | 1 ± 2
Toe angle (per wheel) | 0°00' ± 05'
Toe-out angle on turns (inner wheel when outer wheel at 20°) | 22°00' ± 1°30'
Camber*3 | 0°00' ± 30'
Caster*3 | 3°10' ± 30'
Kingpin inclination angle | 12°05' ± 1°30'
Side slip (per 1m) mm | 0 ± 3
Steering angle | Inner wheels | 34°50' ± 1°30'
Outer wheels (reference) | 29°20'
Rear | Toe-in (at the centre of tyre tread) mm | 3 ± 2
Toe angle (per wheel) | 0°08' ± 05'
Camber | -0°40' ± 30'
Wheels and tyres | Tyre size | 215/60 R16 95H | 215/55 R17 94V
Wheel size | 16 × 6JJ | 17 × 6.5JJ
Offset mm | 46 | 38
NOTE: *1 : Vehicles with over fender. *2 : Vehicles with roof rails. *3 : Difference between right and left wheels must be less than 30'.

[0] GENERAL - - MAJOR SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation