[23B] AUTOMATIC TRANSMISSION OVERHAUL <F4A4/W4A4> - - OIL PUMP - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

OIL PUMP

DISASSEMBLY AND REASSEMBLY
|  |  | Disassembly steps
--- | --- | --- | ---
| >>B<< | 1. | O-ring
|  | 2. | Seal ring
| >>A<< | 3. | Oil seal
|  | 4. | Oil pump
| REASSEMBLY SERVICE POINTS
| >>A<< OIL SEAL INSTALLATION
| Use the special tool Oil seal installer (MD998334) to install the oil seal.
| >>B<< O-RING INSTALLATION Install a new O-ring in the groove on the periphery of the oil pump, and apply ATF, blue petrolatum jelly or white Vaseline to the periphery of the O-ring.

[23B] AUTOMATIC TRANSMISSION OVERHAUL <F4A4/W4A4> - - OIL PUMP - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation