[1] PRE-DELIVERY INSPECTION - - AFTER ROAD TEST - 37. MANUAL TRANSMISSION AND TRANSFER (4WD) OIL LEVEL | PRINT PAGE / INDEX / PRIOR / NEXT

| 37. MANUAL TRANSMISSION AND TRANSFER (4WD) OIL LEVEL Remove the filler plug. Check the oil level. If the oil level is at or slightly below the filler hole, it is in satisfactory condition. If the level is low, replenish the transmission and transfer case with fresh oil by using a lubricator. NOTE: For the specified oil, refer to GROUP 2, Periodic Inspection and Maintenance.

[1] PRE-DELIVERY INSPECTION - - AFTER ROAD TEST - 37. MANUAL TRANSMISSION AND TRANSFER (4WD) OIL LEVEL | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation