[42] BODY - - DOOR - ON-VEHICLE SERVICE - GLASS SLIDING MECHANISM CHECK AND ADJUSTMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| GLASS SLIDING MECHANISM CHECK AND ADJUSTMENT
| If the window glass automatically starts moving downwards at the wrong time while it is being raised, carry out the following adjustment or replacement procedures. Remove the door trim assembly (Refer to GROUP 52A, Door trim ). Remove the waterproof film (Refer to ). Remove the window regulator assembly from the door window glass, and then raise and lower the door window glass by hand to check the operation force. NOTE: Insert a cushion or similar object to prevent damage to the glass if it should happen to fall down.
| If the door window glass does not move up and down smoothly, check or repair the following points. Check the installation condition of the runchannel. Repair any twisting in the door sash. Check the installation condition of the lower sash. If repair or adjustment is not possible, replace the door assembly.

[42] BODY - - DOOR - ON-VEHICLE SERVICE - GLASS SLIDING MECHANISM CHECK AND ADJUSTMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation