[33] FRONT SUSPENSION - - LOWER ARM - BALL JOINT DUST COVER REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| BALL JOINT DUST COVER REPLACEMENT If the dust cover is damaged accidentally during service work, replace the dust cover as follows: Remove the dust cover. Apply specified grease to the lip and the inside of a new dust cover. Specified grease: Multipurpose grease SAE J310, NLGI No.2 or equivalent Grease amount for the inside the dust cover (reference): 8 - 10g
| Using special tool ball Joint remover and installer (MB990800), drive in the dust cover until it is fully seated.
| Position the dust cover as shown in the illustration. Make sure that there is no abnormal bulge or pressure applied on the dust cover. Check the dust cover for cracks or damage by pushing it with your finger.

[33] FRONT SUSPENSION - - LOWER ARM - BALL JOINT DUST COVER REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation