[12] ENGINE LUBRICATION - - ON-VEHICLE SERVICE - ENGINE OIL REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| ENGINE OIL REPLACEMENT Start the engine and allow it to warm up until the temperature of the coolant reaches 80 °C to 90 °C. Remove the engine oil filler cap. WARNING Use care as oil could be hot. Remove the drain plug to drain oil.
| Install a new drain plug gasket so that it faces in the direction shown in the illustration, and then tighten the drain plug to the specified torque. Tightening torque: 39 ± 5 N·m NOTE: Install the drain plug gasket so it faces in the direction shown in the illustration.
| Refill with specified quantity of oil. Specified Engine Oil (API classification): SE or higher Total quantity (Includes volume inside oil filter): 4.3 L NOTE: If SE grade engine oil or higher is difficult to obtain, use API classification SD engine oil. NOTE: SAE 0W-30, 5W-30, and 5W-40 engine oils can only be used if they meet ACEA A3 and API SG (or higher) specifications. Install the engine oil filler cap. Check oil level.

[12] ENGINE LUBRICATION - - ON-VEHICLE SERVICE - ENGINE OIL REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation