[1] BODY CONSTRUCTION - - STIFFENER AND DAMP SHEET APPLICATION LOCATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

STIFFENER AND DAMP SHEET APPLICATION LOCATIONS Sound insulation was improved with anti-vibration effects and heightening surface rigidity with a stiffener on the inner side of the side outer panel, and front fender, as well as a damping sheet adhered to the inner side of the front door. NOTE: The main contents of a stiffener are epoxy resin. It comes in a sheet form and contains a mixture of glass fiber and filler, and cures (stiffens) when heated. It is used to improve the rigidity of the outer plate.

[1] BODY CONSTRUCTION - - STIFFENER AND DAMP SHEET APPLICATION LOCATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation