[13B] MULTIPORT FUEL INJECTION (MPI) <4G64> - - TROUBLESHOOTING - INSPECTION CHART FOR DIAGNOSIS CODE | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION CHART FOR DIAGNOSIS CODE
Code No. | Diagnosis item | Reference page
--- | --- | ---
12 | Air flow sensor system |
13 | Intake air temperature sensor system |
14 | Throttle position sensor system |
21 | Engine coolant temperature sensor system |
22 | Crank angle sensor system |
23 | Camshaft position sensor |
24 | Vehicle speed signal system |
25 | Barometric pressure sensor system |
31 | Detonation sensor system |
41 | Injector system |
44 | Ignition coil (power transistor) system |
64 | Alternator FR terminal system |
NOTE: Do not replace the engine-A/T-ECU until a through terminal check reveals there are no short/open circuit. Check that the engine-A/T-ECU earth circuit is normal before checking for the cause of the problem.

[13B] MULTIPORT FUEL INJECTION (MPI) <4G64> - - TROUBLESHOOTING - INSPECTION CHART FOR DIAGNOSIS CODE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation