[54A] CHASSIS ELECTRICAL - - COMBINATION METER ASSEMBLY AND VEHICLE SPEED SENSOR - ON-VEHICLE SERVICE - ENGINE COOLANT TEMPERATURE GAUGE UNIT CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| ENGINE COOLANT TEMPERATURE GAUGE UNIT CHECK Drain the engine coolant (Refer to GROUP 14- On-vehicle Service ). Remove the engine coolant temperature gauge unit.
| Put water temperature gauge unit into the hot water in specified temperature, and ensure that basic resistance is within standard value. Standard value: 104 ± 13.5 Ω (at 70C°) Reference value
Temperature (°C) | Resistance Ω
--- | ---
50 | 230
60 | 155
80 | 73
| After inspection, apply specified sealant at threads of water temperature gauge unit, and tighten to the specified torque. Semi-drying sealant: 3M 1215 or equivalent Add engine coolant (Refer to GROUP 14 - On-vehicle Service ).

[54A] CHASSIS ELECTRICAL - - COMBINATION METER ASSEMBLY AND VEHICLE SPEED SENSOR - ON-VEHICLE SERVICE - ENGINE COOLANT TEMPERATURE GAUGE UNIT CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation