[55B] AUTOMATIC AIR CONDITIONER - - TROUBLESHOOTING - DIAGNOSIS FUNCTION | PRINT PAGE / INDEX / PRIOR / NEXT

DIAGNOSIS FUNCTION
How to read diagnosis code Connect the MUT-II to the 16-pin diagnosis connector to read diagnosis code (Refer to GROUP 00 How to Use Troubleshooting/Inspection Service Points ).
How to erase diagnosis code Refer to GROUP 00 - How to Use Troubleshooting/Inspection Service Points .

[55B] AUTOMATIC AIR CONDITIONER - - TROUBLESHOOTING - DIAGNOSIS FUNCTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation