[14] ENGINE COOLING - - ON-VEHICLE SERVICE - CONCENTRATION MEASUREMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| CONCENTRATION MEASUREMENT Measure the temperature and specific gravity of the engine coolant to check the antifreeze concentration. Standard value: 30 - 60 % (allowable concentration range) Recommended antifreeze: DIAQUEEN SUPER LONG LIFE COOLANT or equivalent CAUTION If the concentration of the anti-freeze is below 30 %, the anti-corrosion property will be adversely affected. In addition, if the concentration is above 60 %, both the anti-freezing and engine cooling properties will decrease, affecting the engine adversely. For these reasons, be sure to maintain the concentration level within the specified range.

[14] ENGINE COOLING - - ON-VEHICLE SERVICE - CONCENTRATION MEASUREMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation