[1] PRE-DELIVERY INSPECTION - - UNDER HOOD - 12. ELECTRICAL WIRING | PRINT PAGE / INDEX / PRIOR / NEXT

| 12. ELECTRICAL WIRING
| Each electrical wiring harness and connector Check each harness to be correctly routed and securely clipped. Confirm that all connections are tight. Ignition cable Be sure that all ignition cables are firmly attached to the spark plugs, distributor cap (or crank angle sensor) and ignition coil.

[1] PRE-DELIVERY INSPECTION - - UNDER HOOD - 12. ELECTRICAL WIRING | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation