[13A] MULTIPORT FUEL INJECTION (MPI) <4G63> - - ON-VEHICLE SERVICE - COMPONENT LOCATION | PRINT PAGE / INDEX / PRIOR / NEXT

COMPONENT LOCATION
Name | Symbol | Name | Symbol
--- | --- | --- | ---
Air flow sensor (with intake air temperature sensor) <SOHC> | F | Fan controller |
Air flow sensor (with intake air temperature sensor and barometric pressure sensor) <DOHC> | O | Fuel pump relay (1) and (2) | G
A/C relay | G | Idle speed control servo | E
A/C switch | Q | Ignition coil | L
A/C pressure sensor | A | Injectors | K
Camshaft position sensor | M | Manifold absolute pressure sensor <SOHC> | J
Crank angle sensor | I | Manifold differential pressure sensor <DOHC> | B
Detonation sensor | C | Oxygen sensor (front) <SOHC> | T
Diagnosis connector | R | Oxygen sensor (rear) <SOHC> | U
EGR control solenoid valve | D | Oxygen sensor <DOHC> | U
Engine coolant temperature sensor | M | Power steering fluid pressure switch | H
Engine control relay | G | Purge control solenoid valve | D
Engine-A/T-ECU | P | Fuel pump relay (1) and (2) | G
Engine warming lamp (check engine lamp) | S | Throttle position sensor | E

[13A] MULTIPORT FUEL INJECTION (MPI) <4G63> - - ON-VEHICLE SERVICE - COMPONENT LOCATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation