[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - ON-VEHICLE SERVICE - THROTTLE VALVE CONTROL SERVO CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| THROTTLE VALVE CONTROL SERVO CHECK
| OPERATION CHECK Remove the air intake hose from the throttle body. Turn the ignition switch to "ON" position. Operate the accelerator pedal and confirm that the throttle valve is opening and closing accordingly.
| CHECK THE COIL RESISTANCE
| Disconnect the electronically controlled throttle valve connector. Measure the resistance between terminals No. 1 and No. 2 at the throttle valve control servo connector. Standard value: 0.3 - 80 Ω (at 20°C) If resistance is outside the standard value, replace the throttle body assembly.

[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - ON-VEHICLE SERVICE - THROTTLE VALVE CONTROL SERVO CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation