[55B] AUTOMATIC AIR CONDITIONER - - COMPRESSOR ASSEMBLY AND TENSION PULLEY - DISASSEMBLY AND ASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

DISASSEMBLY AND ASSEMBLY
|  |  | Cooling temperature switch disassembly steps
--- | --- | --- | ---
|  | 1. | Snap ring
|  | 2. | Cooling temperature switch
|  | 3. | O ring
|  |  | Magnetic clutch disassembly
| >>D<< | • | Air gap adjustment
<<A>> | >>C<< | 4. | Self-locking nut
|  | 5. | Armature
| >>B<< | 6. | Snap ring
|  | 7. | Rotor
|  | 8. | Snap ring
| >>A<< | 9. | Field core
|  | 10. | Shim
|  | 11. | A/C compressor
| DISASSEMBLY SERVICE POINT
| <<A>> SELF-LOCKING NUT REMOVAL
| Use the special tool to remove the self-locking nut. Special spanner (MB991367) Pin (MB991386)
| ASSEMBLY SERVICE POINTS
| >>A<< FIELD CORE ATTACHMENT
| Line up the pin hole on the compressor unit with the field core projection and attach.
| >>B<< SNAP RING INSTALLATION
| Using snap ring pliers, fit the snap ring so that the snap ring’s tapered part is on the outside.
| >>C<< SELF-LOCKING NUT INSTALLATION
| Use the special tool to install the self-locking nut. Special spanner (MB991367) Pin (MB991386)
| >>D<< AIR GAP ADJUSTMENT
| Apply voltage from the battery to the magnetic clutch and check that the clutch air gap is inside the standard value. If outside the standard value, use a shim to adjust the gap. Standard value: 0.3 - 0.5 mm

[55B] AUTOMATIC AIR CONDITIONER - - COMPRESSOR ASSEMBLY AND TENSION PULLEY - DISASSEMBLY AND ASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation