[51] EXTERIOR - - WINDSHIELD WIPER AND WASHER - SERVICE SPECIFICATION | PRINT PAGE / INDEX / PRIOR / NEXT

WINDSHIELD WIPER AND WASHER

SERVICE SPECIFICATION
Item | Standard value
--- | ---
Stop position of the windshield wiper arm/blade assembly (Distance between the edge of the wiper blade and the end of the deck garnish) mm | Driver’s side: 30 ± 5 Passenger’s side: 65 ± 5

[51] EXTERIOR - - WINDSHIELD WIPER AND WASHER - SERVICE SPECIFICATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation