[54A] CHASSIS ELECTRICAL - - IGNITION SWITCH - IGNITION SWITCH - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

IGNITION SWITCH

REMOVAL AND INSTALLATION
WARNING Before removal of the air bag module, refer to GROUP 52B, SRS Service Precautions () and Air Bag Module and Clock Spring (). When removing and installing the steering wheel, do not let it bump against the air bag module.
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Instrument lower panel (Refer to GROUP 52A, Instrument panel assembly <L.H.drive vehicles> or <R.H.drive vehicles>)
|  | 2. | Steering wheel (Refer to GROUP 37, Steering wheel <2000-SOHC and 2400> or <2000-DOHC>)
|  | 3. | Column cover upper
|  | 4. | Column cover lower
|  | 5. | Clock spring and column switch assembly (Refer to GROUP 52B, Air bag module(s) and clock spring )
<<A>> |  | 6. | Steering lock cylinder
|  | • | Ignition switch connector
|  | 7. | Ignition switch
|  | • | Key reminder switch connector
|  | 8. | Key reminder switch and ring assembly
|  | 9. | Key reminder switch
|  | 10. | Illumination ring
|  | 11. | Key reminder switch and bulb assembly
|  | 12. | Immobilizer-ECU
| REMOVAL SERVICE POINT
| <<A>> STEERING LOCK CYLINDER REMOVAL
| Insert the key in the steering lock cylinder and turn it to the "ACC" position. Using a small Phillips head screwdriver, pull the steering lock cylinder toward you.

[54A] CHASSIS ELECTRICAL - - IGNITION SWITCH - IGNITION SWITCH - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation