[54A] CHASSIS ELECTRICAL - - REAR FOG LAMP <2400 for Hong Kong spec. and Argentina> - REAR FOG LAMP - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| REAR FOG LAMP SWITCH CONTINUITY CHECK
Switch position | Tester connection | Specified condition
--- | --- | ---
Pressed | 1 - 2 | Less than 2 ohms
Released | 1 - 2 | Open circuit
| REAR FOG LAMP RELAY CHECK
Battery voltage | Tester connection | Specified condition
--- | --- | ---
Not supplied | 1 - 4 | Open circuit
Connect terminal 3 to the positive battery terminal Connect terminal 2 to the negative battery terminal | 1 - 4 | Less than 2 ohms

[54A] CHASSIS ELECTRICAL - - REAR FOG LAMP <2400 for Hong Kong spec. and Argentina> - REAR FOG LAMP - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation