[1] PRE-DELIVERY INSPECTION - - UNDER HOOD - 6. ENGINE OIL LEVEL | PRINT PAGE / INDEX / PRIOR / NEXT

UNDER HOOD

| 6. ENGINE OIL LEVEL
| Check that the oil level is between "MAX" and "MIN". If it is at or below MIN, add the necessary amount of the specified engine oil referring to GROUP 2, Periodic Inspection and Maintenance.

[1] PRE-DELIVERY INSPECTION - - UNDER HOOD - 6. ENGINE OIL LEVEL | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation