[42] BODY - - SUNROOF ASSEMBLY - ON-VEHICLE SERVICE - SUNROOF INITIALIZATION | PRINT PAGE / INDEX / PRIOR / NEXT

| SUNROOF INITIALIZATION
| Assemble the roof lid glass assembly and sunroof motor assembly to the sunroof assembly. Connect the sunroof motor assembly connector and sunroof switch connector to the wire ring harness connector on the vehicle side. Fully open the roof lid glass by pressing the sunroof switch, then fully close the sunroof by pressing the close switch again. Continuously press the close switch for a minimum of 3 seconds after the sunroof is fully closed. Press the open switch to fully open the sunroof, then press the close switch to fully close the sunroof. NOTE: Do not stop the sunroof before the sunroof is fully opened or fully closed in Step 5, above. If the fully open or closed operation is interrupted/stopped, start over from Step 3.

[42] BODY - - SUNROOF ASSEMBLY - ON-VEHICLE SERVICE - SUNROOF INITIALIZATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation