[16] ENGINE ELECTRICAL - - CHARGING SYSTEM - ALTERNATOR ASSEMBLY - REMOVAL AND INSTALLATION <4G64-SOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <4G64-SOHC>
Pre-removal Operation Under Cover Removal (Refer to GROUP 51, Under Cover ). Drive Belt Removal (Refer to GROUP 11A, Crankshaft Pulley ). | Post-installation Operation Drive Belt Installation (Refer to GROUP 11A, Crankshaft Pulley ). Drive Belt Tension Adjustment (Refer to GROUP 11A, On-vehicle Service ). Under Cover Installation (Refer to GROUP 51, Under Cover ).
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Oil level gauge and guide
|  | 2. | O-ring
|  | 3. | Control harness connector
|  | 4. | Harness bracket
|  | 5. | Power steering oil pressure hose clamp
|  | 6. | Brake fluid level sensor connector connection
|  | 7. | Brake reservoir tank connecting bolts
|  | 8. | Brake master cylinder connecting nuts
|  | 9. | Brake pipe connection
|  | 10. | Alternator brace
|  | 11. | Water pump pulley
|  | 12. | Alternator connector
<<A>> |  | 13. | Alternator assembly
| REMOVAL SERVICE POINT
| <<A>> ALTERNATOR ASSEMBLY REMOVAL CAUTION Do not jack up the engine more than necessary as the oil pan will be damaged. Jack up the engine.
| Apply a protective tape around the brake lines. Move up the brake master cylinder to create sufficient clearance between it and the intake manifold.
| Remove the alternator assembly as shown.

[16] ENGINE ELECTRICAL - - CHARGING SYSTEM - ALTERNATOR ASSEMBLY - REMOVAL AND INSTALLATION <4G64-SOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation