[54D] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Except for Hong Kong spec.> - - SYMPTOM PROCEDURES - SUNROOF - INSPECTION PROCEDURE F-3: Sunroof timer function does not work normally. <Vehicles for Australia> | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE F-3: Sunroof timer function does not work normally. <Vehicles for Australia>
| CAUTION Whenever the ECU is replaced, ensure that the input and output signal circuits are normal.
| COMMENTS ON TROUBLE SYMPTOM If the sunroof timer function does not work, the input circuit from the ignition switch (IG1) or all the door switches, the communication lines between the ETACS-ECU and the sunroof motor assembly (sunroof-ECU), the sunroof motor assembly (sunroof-ECU) or the ETACS-ECU may be defective.
| POSSIBLE CAUSES Malfunction of ETACS-ECU Malfunction of the door switch Malfunction of the sunroof motor assembly (sunroof-ECU) Damaged harness wires and connectors
| DIAGNOSIS PROCEDURE
| Step 1. Pulse check Check the input signals from the ignition switch (IG1) and all the door switches.
System switch | Check condition
--- | ---
Ignition switch (IG1) | When turned from ACC to ON
All of the door switches | A door is opened when all the doors are closed
OK: The MUT-II/III sounds or the voltmeter needle fluctuates. Q: Is the check result normal? All the signals are received normally.: Go to Step 2. The ignition switch (IG1) signal is not received.: Refer to Inspection Procedure P-2 "The ignition switch (IG1) signal is not received ." All the door switch signals are not received.: Refer to Inspection Procedure P-12 "All the door switch signals are not received. <RH drive vehicles>"
| Step 2. Connector check: D-09 sunroof motor assembly connector Q: Is the check result normal? YES: Go to Step 3. NO: Repair the connector.
| Step 3. Measure the voltage at the D-09 sunroof motor assembly connector. Disconnect the sunroof motor assembly connector, and measure at the harness side. Check the voltage between D-09 sunroof motor assembly connector terminal No.2 and body earth. OK: Battery positive voltage Q: Is the check result normal? YES: Go to Step 5. NO: Go to Step 4.
| Step 4. Check the wiring harness between D-09 sunroof motor assembly connector terminal No.2 and the battery. Check the power supply line for open circuit. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Repair the wiring harness.
| Step 5. Connector check: C-219 ETACS-ECU connector Q: Is the check result normal? YES: Go to Step 6. NO: Repair the connector.
| Step 6. Check the wiring harness between D-09 sunroof motor assembly connector terminal No.10 and C-219 ETACS-ECU connector terminal No.59. NOTE: Prior to the wiring harness inspection, check joint connector C-02 and intermediate connector C-218, and repair if necessary. Check the communication lines for open circuit. Q: Is the check result normal? YES: Go to Step 7. NO: Repair the wiring harness.
| Step 7. Retest the system. Check that the sunroof timer function work normally. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Replace the sunroof motor assembly.

[54D] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Except for Hong Kong spec.> - - SYMPTOM PROCEDURES - SUNROOF - INSPECTION PROCEDURE F-3: Sunroof timer function does not work normally. <Vehicles for Australia> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation