[17] ENGINE AND EMISSION CONTROL - - ENGINE CONTROL - SYMPTOM CHART | PRINT PAGE / INDEX / PRIOR / NEXT

SYMPTOM CHART
Symptom | Inspection procedure | Reference page
--- | --- | ---
Throttle valve will not fully open or close <4G63, 4G64> | 1 |
Throttle valve will not fully open or close <4G69-L.H. drive vehicles> | 2 |
Throttle valve will not fully open or close <4G69-R.H. drive vehicles> | 3 |
Accelerator pedal operation is not smooth (over acceleration) <4G63, 4G64, 4G69-L.H. drive vehicles> | 4 |
Accelerator pedal operation is not smooth (over acceleration) <4G69-R.H. drive vehicles> | 5 |

[17] ENGINE AND EMISSION CONTROL - - ENGINE CONTROL - SYMPTOM CHART | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation