[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - SRS CONTROL UNIT (SRS-ECU) - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION WARNING If any problems are found, replace the SRS-ECU. Check the SRS-ECU and brackets for dents, cracks or deformation. Check the SRS-ECU connector for damage, and the terminals for deformation. NOTE: For the checks other than the items above, refer to "Troubleshooting" (Refer to ).

[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - SRS CONTROL UNIT (SRS-ECU) - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation