[11B] ENGINE OVERHAUL <4G6-SOHC> - - TORQUE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

TORQUE SPECIFICATIONS
Item | N·m
--- | ---
ALTERNATOR AND IGNITION COIL
Auto-tensioner bolt (M10) | 44 ± 10
Auto-tensioner bolt (M8) | 24 ± 4
Water pump pulley bolt | 8.8 ± 1.0
Alternator brace bolt (water pump end) | 23 ± 3
Alternator brace bolt (alternator end) | 22 ± 4
Alternator nut | 44 ± 10
Crankshaft pulley bolt | 25 ± 4
Ignition coil bolt | 10 ± 2
Spark plug | 25 ± 5
Camshaft position sensor bolt | 8.8 ± 1.0
Camshaft position sensor support bolt | 14 ± 1
Camshaft position sensing cylinder bolt | 22 ± 4
TIMING BELT
Timing belt front cover flange bolt (M6) | 11 ± 1
Timing belt front cover flange bolt (M8) | 14 ± 1
Timing belt front cover washer assembled bolt | 9.0 ± 1.0
Power steering pump bracket bolt | 49 ± 9
Crank angle sensor bolt | 8.8 ± 1.0
Tensioner pulley bolt | 48 ± 5
Tensioner arm bolt | 21 ± 4
Auto-tensioner bolt | 23 ± 3
Idler pulley bolt | 35 ± 6
Oil pump sprocket bolt | 54 ± 4
Crankshaft bolt | 167
Tensioner B bolt | 19 ± 3
Counterbalance shaft sprocket bolt | 45 ± 3
Engine support bracket bolt | 49 ± 5
Camshaft sprocket bolt | 89 ± 9
FUEL SYSTEM
Throttle body bolt | 19 ± 3
EGR valve bolt | 20 ± 2
Delivery pipe and injector assembly bolt | 11 ± 1
Fuel pressure regulator bolt | 9.0 ± 1.0
Vacuum pipe and hose bolt | 9.0 ± 1.0
Solenoid valve bolt | 9.0 ± 1.0
INTAKE MANIFOLD
Engine coolant temperature sensor | 29 ± 10
Engine coolant temperature gauge unit | 11 ± 1
Water inlet fitting bolt | 13 ± 2
Thermostat housing bolts | 23 ± 4
Water inlet pipe bolt | 13 ± 2
Water pump bolts | 14 ± 1
Oil level gauge guide bolt | 13 ± 1
Intake manifold stay bolts | 31 ± 3
Manifold pressure sensor bolts | 5.0 ± 1.0
Intake manifold bolts and nuts | 20 ± 2
Detonation sensor | 23 ± 2
EXHAUST MANIFOLD
Water outlet fitting bolts | 13 ± 2
Exhaust manifold cover bolts | 14 ± 1
Engine hanger bolt | 19 ± 3
Exhaust manifold nuts (M8) | 29 ± 3
Exhaust manifold nuts (M10) | 49 ± 5
Oxygen sensor | 44 ± 5
Exhaust manifold brackets bolt (Cylinder block side) | 35 ± 6
Exhaust manifold brackets bolt (Exhaust manifold side) | 44 ± 5
ROCKER ARMS AND CAMSHAFT
Rocker cover bolts | 3.4 ± 0.5
Rocker arm shaft bolts | 31 ± 3
CYLINDER HEAD AND VALVES
Cylinder head bolts | 78 ± 2 → loosen completely →20 ± 2 → 90°+ 90°
FRONT CASE AND OIL PAN
Drain plug | 39 ± 5
Transmission stay bolts | 22 ± 4
Oil pan bolts | 9.0 ± 3.0
Oil pan lower section bolts | 9.0 ± 3.0
Oil pan upper section bolts | 9.0 ± 3.0
Oil screen bolts | 19 ± 3
Oil pressure switch | 19 ± 3
Relief plug | 44 ± 5
Oil filter bracket bolts | 19 ± 3
Plug | 23 ± 3
Flange bolt | 36 ± 6
Front case bolts | 23 ± 3
Oil pump cover bolts | 17 ± 1
Oil pump cover screw | 10 ± 2
PISTONS AND CONNECTING RODS
Connecting rod cap nuts | 20 ± 2 → 90° to 94°
CRANKSHAFT AND CYLINDER BLOCK
Drive plate bolts | 132 ± 5
Rear plate bolt | 11 ± 1
Bell housing cover bolts | 9.0 ± 1.0
Rear oil seal case bolts | 11 ± 1
Bearing cap bolts | 25 ± 2 → 90° to 100°

[11B] ENGINE OVERHAUL <4G6-SOHC> - - TORQUE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation