[17] ENGINE AND EMISSION CONTROL - - ENGINE CONTROL - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICE SPECIFICATIONS
Items | Standard value
--- | ---
Accelerator cable play mm | 1.0 - 2.0
Engine idle speed r/min | 4G63, 4G69 | 750 ± 100
4G64 | 700 ± 100

[17] ENGINE AND EMISSION CONTROL - - ENGINE CONTROL - SERVICE SPECIFICATIONS | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation