[00] GENERAL - - TECHNICAL FEATURES - ACTIVE SAFETY | PRINT PAGE / INDEX / PRIOR / NEXT

ACTIVE SAFETY
BRAKING SYSTEM A 8+9 inch tandem brake booster has been adopted to provide sufficient braking force in sudden braking range. Front ventilate disc brakes have been adopted to provide stabled braking force and improved braking feel. <Except for Hong Kong spec. (2000-DOHC), South Africa and Argentina> 2-piston front ventilate disc brakes have been adopted to provide stable braking force, improved braking feel, and fade-resistant characteristics. <Vehicles for Hong Kong spec. (2000-DOHC), South Africa and Argentina> 9-inch leading trailing-type rear drum brakes have been adopted to provide sufficient braking force in sudden braking range. <Except for Hong Kong spec. (2000-DOHC, 2400), South Africa, Argentina, Australia and New Zealand> 14-inch solid disk brakes have been adopted to provide stable braking force and fade-resistant characteristics. <Vehicles for Hong Kong spec. (2000-DOHC, 2400), South Africa, Argentina, Australia and New Zealand (2400)> A 4-sensor, 3-channel ABS (Anti-lock Braking System) with EBD (Electronic Brake-force Distribution) is available.

[00] GENERAL - - TECHNICAL FEATURES - ACTIVE SAFETY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation