[55B] AUTOMATIC AIR CONDITIONER - - ON-VEHICLE SERVICE - CLEAN AIR FILTER REPLACEMENT PROCEDURE <VEHICLES FOR SOUTH AFRICA> | PRINT PAGE / INDEX / PRIOR / NEXT

| CLEAN AIR FILTER REPLACEMENT PROCEDURE <VEHICLES FOR SOUTH AFRICA> Remove the glove box. (Refer to GROUP 52A - Instrument Panel )
| Remove the two screws as shown, and replace the clean air filter. Remove the clean air filter. Install the glove box.

[55B] AUTOMATIC AIR CONDITIONER - - ON-VEHICLE SERVICE - CLEAN AIR FILTER REPLACEMENT PROCEDURE <VEHICLES FOR SOUTH AFRICA> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation