[42] BODY - - KEYLESS ENTRY SYSTEM - ON-VEHICLE SERVICE - KEYLESS ENTRY SYSTEM CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| ON-VEHICLE SERVICE

| KEYLESS ENTRY SYSTEM CHECK Check the system as described below. If the system does not work, carry out troubleshooting. Refer to GROUP 54B, Troubleshooting , refer to GROUP 54C, Troubleshooting , refer to GROUP 54D, Troubleshooting or refer to GROUP 54E, Troubleshooting . Operate the transmitter to check that the doors and tailgate can be locked and unlocked. Operate the transmitter to check that the answerback function works in response to door and tailgate locking/unlocking. NOTE: The adjustment function allows you to change the answerback setting as follows. Prior to that check, confirm which setting is activated. The hazard warning lamps flash twice when locked and once when unlocked. The room lamp flashes twice when locked and illuminates for 15 seconds when unlocked. The hazard warning lamps do not flash when locked and flash once when unlocked. The room lamp flashes twice when locked and illuminates for 15 seconds when unlocked. The hazard warning lamps flash twice when locked and do not flash when unlocked. The room lamp flashes twice when locked and illuminates for 15 seconds when unlocked. The hazard warning lamps do not flash when both locked and unlocked. The room lamp flashes twice when locked and illuminates for 15 seconds when unlocked.

[42] BODY - - KEYLESS ENTRY SYSTEM - ON-VEHICLE SERVICE - KEYLESS ENTRY SYSTEM CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation