[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T> - ACTUATOR TEST JUDGMENT VALUE | PRINT PAGE / INDEX / PRIOR / NEXT

ACTUATOR TEST JUDGMENT VALUE
Item No. | Inspection item | Test description | Inspection condition | Normal status
--- | --- | --- | --- | ---
01 | LR solenoid valve | Actuate solenoid valve indicated by MUT-II/III for 5 seconds at duty ratio of 50%. Other remaining solenoid valve are not ON. | Ignition switch: ON Selector lever position: P Engine: Stopped Accelerator pedal: Released | When solenoid valve is actuated, operating sound is audible.
02 | UD solenoid valve
03 | 2ND solenoid valve
04 | OD solenoid valve
05 <5A/T> | RED solenoid valve
06 | DCC solenoid valve
07 | 1st indicator lamp | Illuminate shift indicator indicated by MUT-II/III for 3 seconds | Shift indicator is displayed.
08 | 2nd indicator lamp
09 | 3rd indicator lamp
10 | 4th indicator lamp
11 <5A/T> | 5th indicator lamp
12 | A/T control relay | A/T control relay is OFF for three seconds. | Data list No.54 During test: 0 V Normal: System voltage (V)
15 <5A/T> | Downshift forbidden buzzer | Let the ETACS-ECU to sound the downshift forbidden buzzer. | The buzzer sounds.

[23A] AUTOMATIC TRANSMISSION (FF) - - TROUBLESHOOTING <A/T> - ACTUATOR TEST JUDGMENT VALUE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation