[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G64-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - TROUBLESHOOTING - DIAGNOSIS FUNCTION | PRINT PAGE / INDEX / PRIOR / NEXT

| DIAGNOSIS FUNCTION
| METHOD OF READING THE DIAGNOSIS CODE Use the MUT-II/III to read the diagnosis code (Refer to GROUP 00 - How to Use Troubleshooting/Inspection Service Points ).
| METHOD OF ERASING THE DIAGNOSIS CODE Use the MUT-II/III to erase the diagnosis code (Refer to GROUP 00 - How to Use Troubleshooting/Inspection Service Points ).

[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G64-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - TROUBLESHOOTING - DIAGNOSIS FUNCTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation