[00] GENERAL - - HOW TO USE THIS MANUAL | PRINT PAGE / INDEX / PRIOR / NEXT

HOW TO USE THIS MANUAL
INDICATION OF DESTINATION General Export and GCC are used for convenience to indicate destination. "General Export" means territories other than Europe, GCC, Australia, New Zealand, the U.S.A. and Canada. "GCC" indicates countries that are members of the (Persian) Gulf Cooperation Council of nations. "Hong Kong spec." indicates the vehicles for Hong Kong etc..Refer to . In some instances, vehicles with other specifications may be shipped to some countries.
MODEL INDICATIONS The following abbreviations are used in this manual for identification of model types. MPI Indicates the multipoint injection, or engine equipped with the multipoint injection.MIVEC Indicates the mitsubishi innovative valve timing and lift electronic control system.2000Indicates models equipped with the 2,000 mL <4G63> petrol engine.2400Indicates models equipped with the 2,400 mL <4G64, 4G69> petrol engine.SOHCIndicates an engine with the single overhead camshaft.DOHCIndicates an engine with the double overhead camshaft.A/TIndicates the automatic transmission, or models equipped with the automatic transmission.A/CIndicates the air conditioner.

[00] GENERAL - - HOW TO USE THIS MANUAL | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation