[33] FRONT SUSPENSION - - CROSSMEMBER BAR - REMOVAL AND INSTALLATION <2000-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

CROSSMEMBER BAR

REMOVAL AND INSTALLATION <2000-DOHC>
| >>A<< | 1. | Crossmember bar
INSTALLATION SERVICE POINT
>>A<< CROSSMEMBER BAR INSTALLATION Install the crossmember bar so that its identification mark faces towards the underside of the vehicle.

[33] FRONT SUSPENSION - - CROSSMEMBER BAR - REMOVAL AND INSTALLATION <2000-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation