[14] ENGINE COOLING - - ON-VEHICLE SERVICE - FAN CONTROLLER CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| FAN CONTROLLER CHECK
| Remove the fan controller connector. Turn the ignition switch to the "ON" position, and measure the voltage between the harness-side connector terminals. Standard value: System voltage
| Connect the fan controller connector, and disconnect the condenser fan motor connector. Ensure that the A/C switch is off, and start the engine and run it at idle. Measure the voltage between the fan controller-side connector terminals. Standard value: 1V or less WARNING Stay clear of the fan when the fan starts running. Turn the A/C switch to the "ON" position. Measure the voltage between the fan controller-side connector terminals while the fan is running. The voltage should repeat the values below. Standard value: 8.2 ± 2.6 V System voltage ± 2.6 V If the voltage does not repeatedly change as indicated, replace the fan controller.

[14] ENGINE COOLING - - ON-VEHICLE SERVICE - FAN CONTROLLER CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation