[55B] AUTOMATIC AIR CONDITIONER - - PHOTO SENSOR - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION Check that the blower rotation comes down if the photo sensor is covered with hands, when the automatic A/C is operating (in summer sunbeam). If not the rotation comes down, replace the photo sensor.

[55B] AUTOMATIC AIR CONDITIONER - - PHOTO SENSOR - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation