[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - SYMPTOM PROCEDURES - FLASHER TIMER - INSPECTION PROCEDURE L-4: Any of the turn-signal lamps does not illuminate. <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE L-4: Any of the turn-signal lamps does not illuminate. <2400>
| CAUTION Whenever the ECU is replaced, ensure that the input and output signal circuits are normal.
| COMMENTS ON TROUBLE SYMPTOM If any of the turn-signal lamp does not illuminate normally, wiring harness connector(s) or the bulb may be defective.
| POSSIBLE CAUSES Defective turn-signal lamp bulb Damaged harness wires and connectors
| DIAGNOSIS PROCEDURE
| Step 1. Connector check: A-29 <front turn: RH> or A-16 <front turn: LH> headlamp assembly connector <Vehicles without discharge headlamp> or A-48 <front turn: RH> or A-47 <front turn: LH> headlamp assembly connector <Vehicles with discharge headlamp>, A-01 <RH> or A-04 <LH> side turn-signal lamp connector, D-14 <turn: RH> or D-19 <turn: LH> rear combination lamp connector, C-05 <turn-signal indicator lamp> and C-04 <turn-signal indicator lamp (LH)> combination meter connector Q: Is the check result normal? YES: Go to Step 2. NO: Repair the connector.
| Step 2. Check the bulb(s) of the turn-signal lamps or the turn-signal indicator lamps. Check the bulb(s) of the defective lamp. Q: Is the check result normal? YES: Go to Step 3. NO: Replace the bulb(s) of the defective lamp.
| Step 3. Measure the resistance at the A-29 <front turn: RH> or A-16 <front turn: LH> headlamp assembly connector <Vehicles without discharge headlamp> or A-48 <front turn: RH> or A-47 <front turn: LH> headlamp assembly connector <Vehicles with discharge headlamp>, the A-01 <RH> or A-04 <LH> side turn-signal lamp connector, the D-14 <turn: RH> or D-19 <turn: LH> rear combination lamp connector, the C-05 <turn-signal indicator lamp> combination meter connector. Disconnect the connector, and measure at the wiring harness side. Measure the resistance between the defective lamp connector terminal and body earth. Resistance between A-29 <front turn: RH> headlamp assembly connector <Vehicles without discharge headlamp> terminal No.1 and body earth Resistance between A-48 <front turn: RH> headlamp assembly connector <Vehicles with discharge headlamp> terminal No.7 and body earth Resistance between A-16 <front turn: LH> headlamp assembly connector <Vehicles without discharge headlamp> terminal No.1 and body earth Resistance between A-47 <front turn: LH> headlamp assembly connector <Vehicles with discharge headlamp> terminal No.7 and body earth Resistance between A-01 <RH> side turn-signal lamp connector terminal No.1 and body earth Resistance between A-04 <LH> side turn-signal lamp connector terminal No.1 and body earth Resistance between D-14 <turn: RH> rear combination lamp connector terminal No.3 and body earth Resistance between D-19 <turn: LH> rear combination lamp connector terminal No.3 and body earth Resistance between C-05 <turn-signal indicator lamp> combination meter terminal No.12 and body earth OK: 2 Ω or less Q: Is the check result normal? YES: Go to Step 5. NO: Go to Step 4.
| Step 4. Check the wiring harness from A-29 <front turn: RH> or A-16 <front turn: LH> headlamp assembly connector terminal No.1 <Vehicles without discharge headlamp> or A-48 <front turn: RH> or A-47 <front turn: LH> headlamp assembly connector terminal No.7 <Vehicles with discharge headlamp>, A-01 <RH> or A-04 <LH> side turn-signal lamp connector terminal No.1, D-14 <turn: RH> or D-19 <turn: LH> rear combination lamp connector terminal No.3, or C-05 <turn-signal indicator lamp> combination meter connector terminal No.12 to body earth. NOTE: Prior to the wiring harness inspection, check intermediate connector C-29 <side RH>, and repair if necessary. Check the earth wires for open circuit. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Repair the wiring harness.
| Step 5. Connector check: C-217 ETACS-ECU connector Q: Is the check result normal? YES: Go to Step 6. NO: Repair the connector.
| Step 6. Check the wiring harness from the A-29 <front turn: RH> or A-16 <front turn: LH> headlamp assembly connector terminal No.3 <Vehicles without discharge headlamp> or A-48 <front turn: RH> or A-47 <front turn: LH> headlamp assembly connector terminal No.8 <Vehicles with discharge headlamp>, the A-01 <RH> or A-04 <LH> side turn-signal lamp connector terminal No.2, the D-14 <turn: RH> or D-19 <turn: LH> rear combination lamp connector terminal No.6, the C-05 <turn-signal indicator lamp (RH)> combination meter connector terminal No.10 or C-04 <turn-signal indicator lamp (LH)> combination meter connector terminal No.31 to C-217 ETACS-ECU connector terminal No.9 <RH> or 14 <LH>. NOTE: Prior to the wiring harness inspection, check intermediate connector C-29 <side RH>, C-116 <front and side LH> or C-117 <rear LH> and junction block connector C-202 <front, side and rear LH>, C-221 <rear RH> or C-205 <turn-signal indicator lamp>, and repair if necessary. Check the output lines for open circuit. Q: Is the check result normal? YES: Go to Step 7. NO: Repair the wiring harness.
| Step 7. Retest the system. Check that the turn-signal lamps and the indicator lamps illuminate normally. Q: Is the check result normal? The lamps illuminate normally at both high and low beams.: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). The front turn-signal lamps do not illuminate.: Replace the socket. The side turn-signal lamps do not illuminate.: Replace the socket. The rear turn-signal lamps do not illuminate.: Replace the socket assembly. The turn-signal indicator lamps do not illuminate.: Replace the combination meter.

[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - SYMPTOM PROCEDURES - FLASHER TIMER - INSPECTION PROCEDURE L-4: Any of the turn-signal lamps does not illuminate. <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation