0 GENERAL
PRECAUTIONS BEFORE SERVICE
PROTECTING THE VEHICLE
DOING SERVICE WORK IN GROUPS OF TWO OR MORE MECHANICS
REMOVAL AND DISASSEMBLY
SPECIAL TOOLS
PARTS TO BE REPLACED
PARTS
TUBES AND OTHER RUBBER PARTS
LUBRICANTS
BRAKE FLUID
SERVICING THE ELECTRICAL SYSTEM
APPLICATION OF ANTI-CORROSION AGENTS AND UNDERCOATS
PRE-INSPECTION CONDITION
VEHICLE WASHING
MUT-III
IN ORDER TO PREVENT VEHICLES FROM FIRE
ENGINE OILS
©2004 Mitsubishi Motors Corporation