[14] ENGINE COOLING - - SERVICE SPECIFICATION | PRINT PAGE / INDEX / PRIOR / NEXT

SERVICE SPECIFICATION
Item | Standard value | Limit
--- | --- | ---
High-pressure valve opening pressure of radiator cap kPa | 93 - 123 | Minimum 83
Range of coolant antifreeze concentration of radiator % | 30 - 60 | -
Thermostat | Valve opening temperature of thermostat °C | 82 ± 1.5 | -
Full-opening temperature of thermostat °C | 95 | -
Valve lift mm | 8.5 or more | -

[14] ENGINE COOLING - - SERVICE SPECIFICATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation