[15] INTAKE AND EXHAUST - - ON-VEHICLE SERVICE - AIR BY-PASS VALVE CHECK <Turbo> | PRINT PAGE / INDEX / PRIOR / NEXT

| AIR BY-PASS VALVE CHECK <Turbo>
| Remove the air bypass valve. Connect the hand vacuum pump to the nipple of the air bypass valve. Apply a negative pressure of approximately 93 kPa, and check that air tightness is maintained. Also check operation of the valve. Standard value:
Negative pressure | Valve operation
--- | ---
Approximately 53 kPa | It starts opening

[15] INTAKE AND EXHAUST - - ON-VEHICLE SERVICE - AIR BY-PASS VALVE CHECK <Turbo> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation