[55A] HEATER, AIR CONDITIONER AND VENTILATION - - TROUBLESHOOTING - SYMPTOM CHART | PRINT PAGE / INDEX / PRIOR / NEXT

SYMPTOM CHART NOTE: Refer to GROUP 14, Trouble shooting for the condenser fan .
Symptom | Inspection Procedure | Reference Page
--- | --- | ---
When the ignition switch is "ON" the A/C does not operate. | 1. |
Inside/outside air selection is not possible. | 2. |
When the A/C is operating, temperature inside the passenger compartment does not decrease (cool air is not emitted). | 3. |
Blower fan and motor do not turn. | 4. |
Blower air amount cannot be changed | 5. |
The A/C indicator flashes. | 6. |
Defogger function does not operate. | 7. |
Defogger Timer function does not operate. | 8. |
Malfunction of the A/C-ECU power supply system. | 9. |
Condenser Fan does not operate. | 10. | Refer to GROUP 14

[55A] HEATER, AIR CONDITIONER AND VENTILATION - - TROUBLESHOOTING - SYMPTOM CHART | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation