[55A] HEATER, AIR CONDITIONER AND VENTILATION - - VENTILATORS - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

VENTILATORS

REMOVAL AND INSTALLATION
|  |  | Foot duct and rear heater duct removal steps
--- | --- | --- | ---
|  | • | Instrument lower cover (Refer to GROUP 52A - Instrument Panel <L.H. drive vehicles>, <R.H. drive vehicles>).
|  | 1. | Foot duct <driver's side>
|  | • | Glove box (Refer to GROUP 52A, instrument panel <L.H. drive vehicles>, <R.H. drive vehicles>).
|  | 2. | Foot duct <front passenger's side>
|  |  | Defroster nozzle and distribution duct removal steps
|  | • | Instrument Panel (Refer to 52A, Instrument panel <L.H. drive vehicles>, <R.H. drive vehicles>).
|  | 3. | Side defroster duct
|  | 4. | Defroster nozzle
|  | 5. | Distribution duct
|  | 6. | Rear ventilation duct

[55A] HEATER, AIR CONDITIONER AND VENTILATION - - VENTILATORS - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation