[52A] INTERIOR - - SEAT - FRONT SEAT | PRINT PAGE / INDEX / PRIOR / NEXT

SEAT

FRONT SEAT
Genuine leather seats are offered as an option. The driver's seat has a height adjustment mechanism. The seatback frame uses a plate spring to improve fitting, holding and vibration resistance and enhance comfort. The driver's seat has a lumbar support adjustment mechanism to reduce fatigue during long drives <L.H. drive vehicles - GLS>. Adopting the four level angle-comfortable large-size armrest for the driver's seat improves ride comfort <R.H. drive vehicles>. The rear collision protection seat mechanism (installation of the seat back frame at the rear and head restraint position optimisation) improves safety in the event of a rear collision at low speeds. The front seat has a seatback pocket (driver’s side <Vehicles for South Africa and Argentina>, passenger’s side). The standard type head restraints <20V, GLX (Except vehicles for South Africa) and LS> or the see-through type head restraints <Except 20V, GLX (vehicles for South Africa) and LS> is installed. Adjusting to up and down optimises the head restraints position. Adjusting to back and forth <Vehicles for South Africa, Argentina> optimises the head restraints position. Heated seats are available for the driver's and passenger's seats. <Option - Vehicles for Argentina>
SPECIFICATIONS FOR HEATED SEAT
ITEM | SPECIFICATIONS
ENERGY CONSUMPTION W | HIGH | 60 ± 6
LOW | 15 ± 2
THERMOSTAT °C | ON→OFF | 40 ± 4
OFF→ON | 30 ± 5
HEATED SEAT SYSTEM CIRCUIT DIAGRAM

[52A] INTERIOR - - SEAT - FRONT SEAT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation