[51] EXTERIOR - - WINDSHIELD WIPER AND WASHER - WINDSHIELD WASHER - REMOVAL AND INSTALLATION <2000> | PRINT PAGE / INDEX / PRIOR / NEXT

WINDSHIELD WASHER

REMOVAL AND INSTALLATION <2000>
|  |  | Windshield washer nozzle removal steps
--- | --- | --- | ---
|  | • | Connection of windshield washer hose
|  | 1. | Windshield washer nozzle
|  |  | Front washer hose removal steps
|  | • | Hood insulator (Refer to GROUP 42, Hood ).
|  | 1. | Windshield washer nozzle
|  | 2. | Front washer hose
|  |  | Washer tank and washer motor removal steps
|  | • | Washer motor connector connection
|  | • | Connection of front washer hose and rear washer hose
|  | 3. | Washer tank assembly
|  | 4. | Windshield washer motor
|  | 5. | Rear washer motor
|  | 6. | Washer tank
NOTE: For removal and installation of the wiper and washer switch, refer to GROUP 54A, Column switch .

[51] EXTERIOR - - WINDSHIELD WIPER AND WASHER - WINDSHIELD WASHER - REMOVAL AND INSTALLATION <2000> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation