[51] EXTERIOR - - OUTSIDE MIRROR - DOOR MIRROR - INSPECTION <Except vehicles for Hong Kong> | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION <Except vehicles for Hong Kong>
| ELECTRIC REMOTE CONTROL MIRROR OPERATION CHECK
| Check that the mirror moves as described in the table when each terminal is connected to the battery.
Battery connection | Direction operation
--- | ---
Connect terminal 5 to the negative battery terminal. Connect terminal 7 to the positive battery terminal. | Up
Connect terminal 5 to the positive battery terminal. Connect terminal 7 to the negative battery terminal. | Down
Connect terminal 5 to the negative battery terminal. Connect terminal 6 to the positive battery terminal. | Right
Connect terminal 5 to the positive battery terminal. Connect terminal 6 to the negative battery terminal. | Left
| DOOR MIRROR CONTROL SWITCH CONTINUITY CHECK
Switch position | Tester connection | Specified condition
--- | --- | ---
OFF | 9 - 2, 9 - 3, 9 - 6, 9 - 10, 9 - 11, 1 - 2, 1 - 3, 1 - 6, 1 - 10, 1 - 11 | Open circuit
Left side | OFF | 9 - 6, 9 - 10, 9 - 11, 1 - 6, 1 - 10, 1 - 11 | Open circuit
Up | 1 - 6, 9 - 11 | Less than 2 ohms
Down | 1 - 11, 6 - 9
Right | 1 - 6, 9 - 10
Left | 1 - 10, 6 - 9
Right side | OFF | 9 - 2, 9 - 3, 9 - 6, 1 - 2, 1 - 3, 1 - 6 | Open circuit
Up | 1 - 6, 3 - 9 | Less than 2 ohms
Down | 1 - 3, 6 - 9
Right | 1 - 6, 2 - 9
Left | 1 - 2, 6 - 9

[51] EXTERIOR - - OUTSIDE MIRROR - DOOR MIRROR - INSPECTION <Except vehicles for Hong Kong> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation