[54A] CHASSIS ELECTRICAL - - IGNITION SWITCH - IGNITION SWITCH - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| IGNITION SWITCH CONTINUITY CHECK
| Disconnect ignition switch connector C-303 without removing the ignition switch. Then check the continuity.
Switch position | Tester connection | Specified condition
--- | --- | ---
"LOCK" (OFF) | 1 - 2, 1 - 3, 1 - 4, 1- 5, 1 - 6, 2 - 3, 2 - 4, 2- 5, 2 - 6, 3 - 4, 3- 5, 3 - 6, 4- 5, 4 - 6, 5 - 6 | Open circuit
"ACC" | 1 - 6 | Less than 2 ohms
"ON" | 1 - 2, 1 - 4, 1 - 6, 2 - 4, 2 - 6, 4 - 6 | Less than 2 ohms
"START" | 1 - 2, 1 - 5, 2 - 5 | Less than 2 ohms
| KEY REMINDER SWITCH CONTINUITY CHECK
| Disconnect key reminder switch connector C-304 without removing the ignition switch and key reminder switch. Then check the continuity.
Status of ignition key | Tester connection | Specified condition
--- | --- | ---
Removed | 4 - 6 | Less than 2 ohms
Inserted | 4 - 6 | Open circuit

[54A] CHASSIS ELECTRICAL - - IGNITION SWITCH - IGNITION SWITCH - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation