[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - SYMPTOM PROCEDURES - FLASHER TIMER - INSPECTION PROCEDURE L-2: The hazard warning lamps do not illuminate. | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE L-2: The hazard warning lamps do not illuminate.
| CAUTION Whenever the ECU is replaced, ensure that the input and output signal circuits are normal.
| COMMENTS ON TROUBLE SYMPTOM If the hazard warning lamps do not illuminate, the hazard warning lamp input signal circuit or the ETACS-ECU may be defective.
| POSSIBLE CAUSES Malfunction of the hazard warning lamp switch Malfunction of the ETACS-ECU Damaged harness wires and connectors
| DIAGNOSIS PROCEDURE
| Step 1. Check that the turn-signal lamps operate. Check that the turn-signal lamps illuminate normally. Q: Is the check result normal? YES: Go to Step 2. NO: Refer to inspection procedure L-1 "The turn-signal lamps do not illuminate" .
| Step 2. Check the power supply circuit. When the ignition switch is at the LOCK (OFF) position, check that the functions below work normally. Ignition key reminder function Lamp reminder function Central door locking system Dome lamp (excluding interior lamp automatic shutdown function) Q: Is the check result normal? YES: Go to Step 3. NO: Refer to inspection procedure A-2 "Check the battery power supply circuit to the ETACS-ECU ."
| Step 3. Pulse check Check the input signal from the hazard warning lamp switch.
System switch | Check conditions
--- | ---
Hazard warning lamp switch | When the hazard warning lamp switch is turned from off to on
OK: The MUT-II/III sounds or the voltmeter needle fluctuates. Q: Is the check result normal? YES: Go to Step 4. NO: Refer to inspection procedure P-12 "The hazard warning lamp switch signal is not received" .
| Step 4. Retest the system. Check that the hazard warning lamps illuminate. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Replace the ETACS-ECU.

[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - SYMPTOM PROCEDURES - FLASHER TIMER - INSPECTION PROCEDURE L-2: The hazard warning lamps do not illuminate. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation